The FSISample2 application demonstrates the handling of commands
in the FSI SDK.

Extensions to FSISample1: 
- collection of items and items types
- give the ability to send a command to POINTs (the restrictions to points is only for demonstration)
 
restrictions:
command parameters are not shown in that sample

Configuration:
Adapt the default config values in Main() according to your own  
network configuration.
(The default values in this sample application correspond to the 
example values in the FPA-5000 Networking Guide document.)


Pre-conditions to build and run the sample:

- Copy the content of the SDKs \Bin directory into the .\sdk directory to run the sample.
- If necessary remove all versions of FSM5000FSI from the directory except the one that
  fits to the version of your test panel.
- Adopt the references to FSM5000FSILoader and FSM5000FSIAPI in the project file 
  (both files located in .\sdk after copying)
- Change the hardcoded settings on top of function Run() to fit your test configuration.
- If you want to have more detailed trace output you may change the line
   fsi.SetTraceLevel(SourceLevels.Warning); 
  into
   fsi.SetTraceLevel(SourceLevels.Verbose); 





