The FSISample1 application demonstrates the 
   - instantiation,
   - configuration,
   - tracing,
   - Panel synchronisation mechanism
   - Panel event synchronisation mechanism
  of the FSI SDK.
 

Pre-conditions to build and run the sample:

To use the sample you have to copy the DLLs delived as FSM5000FSI 
to the "sdk" subfolder. Adapt the references to FSM5000FSI and 
FSM5000FSIAPI in the FSISample1 solution (both files are located in 
.\sdk after copying). Otherwise you will get compiler errors about 
missing references.
 
Adapt the default config values in Main() according to your own  
network configuration.
(The default values in this sample application correspond to the 
example values in the FPA-5000 Networking Guide document.)

If you want to have more detailed trace output you can change the line
   fsi.SetTraceLevel(SourceLevels.Warning); 
  into
   fsi.SetTraceLevel(SourceLevels.Verbose); 
